=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Pointe des Galets   451/001 RLR(1979) is 9.5m below Repere A
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Aug-2010
Tide gauge was re-instated in 2007. Previous TGBM was BM A 3.0m above Chart Datum. TGBM is now IGN AMO 2.809m above Chart Datum. Chart Datum has remained the same as confirmed by Ronan Creach email of 19.08.10. Therefore RLR factor remains 6.500m.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Mar-2012
Now that there are several years of data for Pointe des Galets following its re-installation the data 2007 onwards appears to be higher than previously. Because of its remote location it is difficult to confirm this one way or the other.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Sep-2014
Using values from the SONEL website the latitude and longitude for Pointe des Galets have been revised. The data downloaded from SONEL included additional data for the 1960's and 2000's. These have been added to the database.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 15-Jul-2025
Updated the whole dataset to ensure they include all the historical data recovered recently by SHOM and the calculated monthly and annual means match those distributed by SONEL.

