=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-May-1995
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-May-1996
Revised data for 1985-1986 received from the National Tidal Centre, Bureau of Meteorology, South Australia
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Aug-2010
Data supplier have confirmed tide gauge zero of datum is Chart Datum, and benchmark DOT 001 is 3.499 m above Chart Datum. RLR (2008) has been defined as 8.8 m below DOT 001
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Feb-2021
The latest data available to download from the NTC for Lucinda is that for 2019.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Feb-2021
The latest data from the NTC available for download for Onslow is that for 2019.

