=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Tema                410/016 RLR(1969) is 9.6m below BM PL8/5
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Tema                410/016 RLR(1969) is 9.6m below BM PL8/5
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 01-Nov-1995
replacement tide gauge installed in 1991: OTT type X(20.102)
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 06-Feb-2002
(New) Tema gauge installed in 1991, but had operating
problems and then the gauge was stolen.

