=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Sep-2002
A description of the sea level network in Finland can be found
in 'Operational Oceanography: Implementation at the European
and Regional scales.  2002 (pp.129-137)'.
PRIOR TO 1971 FCODE=06
PRIOR TO 1977 GAUGE AT 64 42 N, 24 30 E CLAIMED CONNECTABLE
This station was formerly known as Hornankallis in the Publication Scientifique.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 04-Jan-2012
From levelling information supplied by the Finnish Meteorological Institute 
gauge site lat. and long and BM details as follows:
1922-1976  64 42 24 30    1294Y
1977-1996  64 39 24 25    83151
The above two benchmarks refer to the old tide gauge.
1997-      64 40 24 24    92409 (1992)
                          95403 (1995)
It was decided to refer to 92409 (1992) as the Primary Benchmark as it also 
appears in the levelling report for 2006 whereas 95403 (1995)does not.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 31-Jan-2017
Following the 2016 levelling exercise some adjustments have been made to the benchmark reference heights - at Raahe this was -1mm for BM 95403. The adjustments are a result of more accurate measuring and calculations using the N2000 height system. The RLR diagram has been re-drawn because of this.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Nov-2019
From 2018 onwards the averages of the Finnish sea level data will be based on 1 min observations. Values are calculated in Finnish normal time (EET).
The data are relative to the reference surface of the Finnish sea level observations and thus the datum is the tide gauge zero.

