=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Thessaloniki        290/051 RLR(1981) is 9.2m below BM R16
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Thessaloniki        290/051 RLR(1981) is 9.2m below BM R16
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Nov-2006
Whole dataset flagged due to unresolved datum query.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 09-Apr-2008
Since the change in the method of sea level recording from
measuring downwards to the usual measuring upwards the tidal
plot for Thessalonika had appeared in error as there seemed
to be a large upwards jump. Following lengthy correspondence
with the HNHS it transpires that following a datum control
and levelling exercise a correction of +0.34m was applied
to the TGZ. When this correction was applied the data
plot appears to be OK.See Greek letter in reply to the letter of 26th March 2007.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 13-Aug-2013
The Hellenic Navy have recently supplied datum diagrams for each of there stations. Previously used benchmark R 16 does not appear on the new diagram. In consequence the RLR diagram has been re-drawn using benchmark R. As a result the RLR factors have changed.

