=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Galveston II        940/008 RLR(1964) is 8.6m below BM35
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 29-Jul-1993
Many stations on the Gulf coast have large values for September 1961.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 14-Jul-1994
For a discussion of submergence near to Galveston, Freeport and Sabine Pass, see Emery and Aubrey (Sea Levels, Land Levels and Tide Gauges), 1991, Springer-Verlag, page 39.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Jan-2000
Galveston was inundated by a major storm on 8 September 1900.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Jul-2011
Data is downloaded from the NOAA website. Datum information was also downloaded NOAA Benchmark was previously labelled as BM 35. Benchmark appears on the NOAA website as 7.151 alias 35.

