DATA FROM 1966 ONWARDS LOOKS IRREGULAR AND UNRELIABLE
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Takoradi            410/001 RLR(1970) is 9.2m below BM GCSH4
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 01-Nov-1995
Gauge type is a Baldwin Lathanis, installed in 1926 1992-95 problems with gauge reported
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 03-Jun-1996
Gauge reported on 17 January 1996 as not operational because of its age.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 10-Mar-2009
2007/8 one minute sea level data downloaded from the IOC Sea Level Station Monitoring Facility Ostend. This is then converted to 15min. data for processing. 2007/8 monthly and annual mean sea level values have now been extrapolated from the data. As the relationship for the prime bench mark remains the same there is no need to alter RLR. Details of the bench marks has been derived from site installation information. Copies of these have been included in the port files and RLR file for reference.

