=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Kuantan Port        550/014 RLR(1986) is 10.7m below BM No C0331
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Kuantan Port        550/014 RLR(1986) is 10.7m below BM No C0331
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 21-Jan-1997
1995 data revised January 1997
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 19-Sep-2012
Publication Tidal Observation Records 2010 confirms that the Primary benchmark 
remains BM C0331 6.496m above TGZ.

