Station moved - new data held in station 643/025
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Kobe                643/024 RLR(1968) is 8.8m below Attached BM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 15-Jul-1994
See comments for Osaka (643/021) and see also those of Emery and Aubrey (Sea Levels, Land Levels and Tide Gauges) 1991 (Springer-Verlag) on subsidence in the Osaka-Kobe area.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 21-Feb-1997
February 1997: data 1984-92 recoded as 643/024 (from 643/025)on advice of authority
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 26-Mar-2002
Kobe gauge replaced 1st January 1984.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 26-Mar-2002
Kobe ceased operating 1992 and was replaced by Kobe II (643/025).

