=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Rauma/Raumo         060/121 RLR(1964) is 7.7m below BMP3
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Rauma/Raumo         060/121 RLR(1964) is 7.7m below BMP3
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Sep-2002
A description of the sea level network in Finland can be found
in 'Operational Oceanography: Implementation at the European
and Regional scales.  2002 (pp.129-137)'.
PRIOR TO 1971 FCODE=06
PRIOR TO 1983 GAUGE AT 61 08 N, 21 27 E
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 09-Jan-2012
The tide gauge at Rauma was moved during 1983. Levelling information recently
supplied by the Finnish Meterological Institute confirms that benchmark P3 no
longer exists. Primary benchmark is now 92403 4.089m above the gauge datum.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Nov-2019
From 2018 onwards the averages of the Finnish sea level data will be based on 1 min observations. Values are calculated in Finnish normal time (EET).
The data are relative to the reference surface of the Finnish sea level observations and thus the datum is the tide gauge zero.

