=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-May-1995
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Mar-1996
SEAFRAME station installed 23/06/1992
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 10-Apr-2000
This is a "baseline station" of the Australian National Tidal Facility.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 10-Apr-2000
Port Stanvac        680/298 RLR(2000) is 9.622m below BM6627/15929
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Oct-2011
Using metadata from the National Tidal Centre, Australia Port Stanvac has been made RLR. Primary benchmark is 6527/8394 SEAFRAME sensor benchmark. 7.578m above Tide Gauge Zero (TGZ). TGZ is 1.280m below AHD (prior to 2008 TGZ was 1.2641m below AHD). The tide gauge was removed at the end of 2010.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 23-Jan-2019
Information from the NTC website:- "The SEAFRAME at Port Stanvac was removed in November 2010 to allow Mobil Refining Australia to decommission the oil refinery. Re-establishment of a tide gauge near Port Stanvac is being investigated".

