NOTICEABLE METEOROLOGICAL INFLUENCES
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Mar del Plata(Club) 860/101 RLR(1977) is 11.8m below Repere No 11
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Mar del Plata(Club) 860/101 RLR(1977) is 11.8m below Repere No 11
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-Aug-1999
station is equipped with both float gauge and NGWLMS system
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 21-Mar-2001
Acoustic gauge installed 1992, alongside existing float gauge.
Mid 1998 - tide gauge found to be left dry after dredging works.
May 1999 gauge relocated 5km south, within Naval Base.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 09-Jan-2002
Mar del Plata (Club) gauge (38 03 S, 57 33W) moved to
Mar del Plata (Naval Base) (38 02'S, 57 31'W) December
1998 because of beach works.  New site levelled into
old benchmark (Repere No.11) and data treated as continuous.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 01-Feb-2023
Mar del Plata (Base Naval) station was moved back to Mar del Plata (Club) tide gauge. 

