=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Degerby             060/281 RLR(1964) is 9.5m below BM1849C
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Degerby             060/281 RLR(1964) is 9.5m below BM1849C
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Sep-2002
A description of the sea level network in Finland can be found
in 'Operational Oceanography: Implementation at the European
and Regional scales.  2002 (pp.129-137)'.
PRIOR TO 1971FCODE=06
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 03-Jan-2012
This station is now more commonly referred to as Foglo. Former Primary
benchmark 1849 c is now no longer used. Benchmark 73125 3.355m relative to 
gauge datum was added in 1973. While benchmark 75400 3.964m relative
to gauge datum was added in 1975.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Nov-2019
From 2018 onwards the averages of the Finnish sea level data will be based on 1 min observations. Values are calculated in Finnish normal time (EET).
The data are relative to the reference surface of the Finnish sea level observations and thus the datum is the tide gauge zero.

