=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-May-1995
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 17-May-1996
Revised  data for 1966-1985 recived from the National Tidal Centre, Bureau of Meteorology, South Australia
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 22-Jan-1998
Formerly known as Bundaberg.  The GLOSS Handbook Station sheets refer to Burnett Heads 1960-76: float/stilling well gauges at different locations on same wharf 1976-79: float/stilling well gauge on Tug Berth Queensland Beach Protection Authority operate analogue and digital recorders at Burmett Heads 2.5km away.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 22-Jan-1998
Gauge type is currently a float/stilling well type
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-May-2002
Anomalously high value for February 1971.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-May-2002
Bundaberg, B. Heads 680/073 RLR(2000) is 11.061m below BM PSM 3853 From documentation downloaded from NTC the primary benchmark remains PSM 3853 6.061m above the datum

