=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Christmas Island II 770/022 RLR(1983) is 9.5m below BMUH-1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 07-Oct-1996
(1974-present) Leupold and Stevens Analog-to-Digital Recorder (ADR);(11/1982-present) Handar Encoder (ENC)Primary gauge: ADR:1974-90, ENC 1991-
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 14-Oct-2013
Complete dataset Feb 1974 to April 2012 was loaded onto the database from UHSLC
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 23-Jun-2014
Using benchmark information supplied by UHSLC the RLR diagram has been revised. Primary benchmark is now UH2 3.17m above the gauge datum. As a result the RLR factor has changed from 6.476m to 6.330m.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 29-Oct-2015
Complete updated JASL data through to 2014 has been loaded onto the database.

