Station moved - new data held in station 646/042
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Ishigaki            646/041 RLR(1976) is 12.6m below Attached BM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Ishigaki            646/041 RLR(1976) is 12.6m below Attached BM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 26-Mar-2002
Isihigaki ceased operating 1986, and was replaced by
Ishigaki II (646/042) 1st October 1986.

