=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Oulu/Uleaborg       060/011 RLR(1964) is 9.7m below BM116
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 21-Jul-1998
21 July 1998: RLR redefined following review of data revisions
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Sep-2002
A description of the sea level network in Finland can be found in 'Operational Oceanography: Implementation at the European and Regional scales.  2002 (pp.129-137)'.
1889-1921 VALUES BASED ON 1 READING PER DAY
1922-1970 VALUES BASED ON 6 READINGS PER DAY
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 09-Jan-2012
Levelling information recently supplied by the Finnish Meteorological Institute confirms that the Primary benchmark remains 116 4.231m above the datum for 1913 onwards. This also brought attention to a previous error in the documentation. The relationship between BM 116 and RLR was quoted as being 9.5m when infact it should be 9.7m.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 04-May-2017
Primary benchmark is now TGBM 04006  as the previous Primary benchmark TGBM 116 was destoyed during construction work.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Nov-2019
From 2018 onwards the averages of the Finnish sea level data will be based on 1 min observations. Values are calculated in Finnish normal time (EET).
The data are relative to the reference surface of the Finnish sea level observations and thus the datum is the tide gauge zero.

