=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 26-Aug-2010
Manzanillo is now RLR. both the benchmark ICH-5 and TGZ are referred to the Geodesic National Datum (GND). ICH-5 is 1.576m above GND while TGZ is 1.42m below GND. Data is referred to TGZ and RLR factor is 4.004m
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 03-Mar-2016
To reflect the fact that the monthly means supplied refer to TGZ and not GND the RLR diagram has been redrawn. As a result the RLRFAC has changed from 4.004m to 5.504m. RLR (2007) is now 8.5m below TGBM ICH-5.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 29-Jun-2016
Information supplied by Cuba confirms that since 1992 the tide gauge sensor is a float recording hourly.

