=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Nov-1992
KOPER      279/002 RLR(1964) IS 8.9 M BELOW BM 5486
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 13-Sep-1993
1991 NEW INSTRUMENT INSTALLED
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 14-Jul-1994
Anomalously low value for September 1979 correct as received from
authority.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jan-1996
Tide gauge of the Hydrometeorological Institute of the
Republic of Slovenia
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jan-1996
Gauge=Matra (KOVO, Praha) until May 1978 when substituted by new
system= Seba-Bandschreiberpegel Delta (Seba Hydrometrie, Germany)
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jan-1996
data up to 1964 supplied by auth 25
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jan-1996
PRIOR TO 1990 DATA FROM AUTH 26
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 18-Dec-1997
data for 1990 received from authority code E1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Jan-1998
data for 1992 onwards from new gauge; data up to 1991 from gauge at
45 33 N  13 44 E
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Apr-1998
Data for 1992 onwards is from gauge at Luka Koper, see station 279/003
Koper is an historic station last data 1991

