=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Hamina              060/361 RLR(1964) is 7.8m below BM PM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Hamina              060/361 RLR(1964) is 7.8m below BM PM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 21-Jul-1998
21 July 1998: RLR redefined following review of revised data
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Sep-2002
A description of the sea level network in Finland can be found
in 'Operational Oceanography: Implementation at the European
and Regional scales.  2002 (pp.129-137)'.
PRIOR TO 1971 FCODE=06
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 09-Jan-2012
From levelling information recently supplied by the Finnish Meteorological
Institute it has been confirmed that the Primary benchmark remains PM 2.75m
above the gauge datum.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Nov-2019
From 2018 onwards the averages of the Finnish sea level data will be based on 1 min observations. Values are calculated in Finnish normal time (EET).
The data are relative to the reference surface of the Finnish sea level observations and thus the datum is the tide gauge zero.

