=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-May-1995
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Sep-2010
Tide gauge bench mark PSM 38627 is 18.040 above tide gauge zero (LAT). RLR (2009) is defined as 21.6 m below PSM 38627
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 04-Feb-2021
Lastest available data from the NTC for station Hay Point was that for 2019.

