=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Zlarin              280/017 RLR(1985) is 9.3m below BM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Zlarin              280/017 RLR(1985) is 9.3m below BM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jan-1996
gauge discontinued 2 June 1988

