=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Bergen              040/221 RLR(1964) is 9.7m below BM B33 N90
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 14-Dec-1992
UP TO 1986 ACODE=03
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Mar-1995
tide gauge network modernised, new equipment installed in 1988
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 19-Jul-2010
The dataset for Bergen has been revised. According to the Norwegian website the dataset begins 01/01/1915. However PSMSL hold data for 1883-1889 this does not appear on the Norwegian website.Primary bench mark is B33 N202 at 2.963m above TGZ. RLR was recalculated using 2008 as the RLR year. The revised RLR factor is 6.937m. RLR (2008) is 9.9m below TGBM B33 N202.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Sep-2012
For information on see level rise along the Norwegian coast see paper "Contributions to sea level variability along the Norwegian coast for 1960-2010" by K Richter, J.E.O. Nilsen and H Drange.

