=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Port Irene          660/003 RLR(1992) is 10.6m below BM 1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Mar-1999
gauge type = Ott
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-Oct-2009
2006 is the last data received from Port Irene as the
tide gauge has been removed due to development of the pier.
A replacement gauge has been established at San Vicente.

