=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Rikitea             808/001 RLR(1983) is 8.8m below BM#3
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Nov-1993
1969-JUNE 1975 supplied by SHOM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 08-Oct-1996
Instrument type: Bristol Bubbler (BUB) (1969-6/1975); Fischer and Porter Analog-to-Digital Recorder (ADR) (6/1975-  )
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 14-Oct-2013
Complete dataset Oct. 1969 to April 2012 downloaded onto the database from UHSLC
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Feb-2014
SHOM has confirmed that the current tide gauge at Rikitea belongs to UHSLC. However, SHOM work closely with UHSLC to maintain and control the instrumentation. SHOM has also recently installed a tide gauge which, longterm will replace the UHSLC gauge.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Oct-2015
Using updated JASL data the complete dataset has been reloaded. Using information from the UH levelling sheet benchmark BM 1 stable primary benchmark since 2001 has been added to the RLR diagram. BM 1 is 1.913m above the datum.

