=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-May-1995
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Aug-2010
Data supplier confirmed tide gauge benchmark PSM 8295 is 5.103 m above tide gauge zero (LAT). RLR (2009) has been defined as 10.2 m above PSM 8295
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Feb-2021
Last data available from the NTC for station Shute Harbour 2 is that for March 2018.

