=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 13-Nov-1991
Data for 1969 was supplied by the National Tidal Centre, Bureau of Meteorology, South Australia based on hourly values
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-May-1995
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
Data for 1961-1962 was supplied by Australian Ocean Data Centre N.S.W.These data are based on High and Low water readings.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Mar-1996
Revised data for 1985-1990 was supplied by the National Tidal Centre, Bureau of Meteorology, South Australia. SEAFRAME station installed 04/09/92. Cocos (Keeling) Is. is a cooperative station between NTF and NOAA/NOS
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-Jan-1998
1985-1992: gauge type=Float/well system Stevens analog-to-digital recorder
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 21-Jan-1998
1961-65: float/stilling well gauge located on original jetty West Is. 1968-71 float/stilling well gauge located near jetty, West Is.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 10-Apr-2000
This is a "baseline station" of the Australian National Tidal Facility.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 10-Apr-2000
Cocos Is.(Home Is.) 680/521 RLR(1996) is 8.604 below PSM101
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Oct-2011
Using metadata from the National Tidal Centre, Australia the RLR diagram has been revised. Primary benchmark is SEAFRAME sensor benchmark 3.554m above Tide Gauge Zero (TGZ). RLR factor is 6.20m.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 23-Jan-2019
Data values for March, May, July, August and September 2016 have been revised.

