=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Nice                230/081 RLR(1988) is 8.7m below Fundamental BM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-Mar-1998
Gauge not in use since the beginning of 1995.  A replacement is planned
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 31-Aug-2000
Nice acoustic gauge installed 18/03/1998.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 17-Oct-2000
Data now supplied by Service Hydrographique et Ocean. de la Marine, Brest.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 29-Mar-2012
Primary benchmark is now NGF M.A.I3K3 - OB 7.712m above TGZ.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 01-Oct-2014
Using data from SONEL the latitude and longitude for Nice have been revised.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 21-Jun-2016
When adding the 2015 data to the dataset it was noted that the value for the datapoint for September 2012 had been revised.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 15-Jul-2025
Updated the whole dataset to ensure they include all the historical data recovered recently by SHOM and the calculated monthly and annual means match those distributed by SONEL.

