=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 04-Mar-1992
Prior to 1990 data from Hidrografski Institut, Split
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 14-Jul-1994
Values for February - March 1958 and November - December 1960 seem low compared to Trieste. Values correct as received from authority.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jan-1996
Tide gauge of the State Hydrographic Institute at Split
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jan-1996
Gauge=A. Ott, Kempten
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 25-Jan-2000
Rovinj              280/006 RLR(1964) is 11.9m below BM = Contact Point
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-Jan-2011
From station report tide gauge at Rovinj operational from 1955 onwards. Primary benchmark BP 82 is 5.820m above TGZ. Benchmark AP 807 is 4.106m above TGZ. RLR factor is 6.080m.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 14-Mar-2019
Referring to the comment of 1994-07-14 dataplots for both Trieste id. 154 and Rovinj have been plotted. The comparison is generally good. Because of this the previous data flags have been removed.

