=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Port Nolloth        430/021 RLR(1963) is 11.8m below BM CDM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Aug-1996
For discussions of MSL changes and extreme sea levels around Namibia and South Africa, see: G.B.Brundrit, S.Afr.J.Mar.Sci.,16,9-17,1995 and S.Searson and G.B.Brundrit, S.Afr.J.of Science, 91,579-588,1995. 1959 - 1972 values based on 8 readings per day.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jun-2000
Data for 1991 deleted as clearly anomalous.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 14-Jun-2000
Data for 1993 deleted as clearly anomalous.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 07-Aug-2006
Following the recent supply of data from the South African Hydrographic Office the data for 2000 has now been revised with official figures.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Sep-2009
Heights of chart datum relative to land levelling datum in South Africa and Namibia: Port Nolloth Datum: up to 31st Dec 1993= -0.718 Datum: 1st Jan 1994 - 31st Dec 1997 = -0.900 Datum: 1st Jan 1998 - 31st Dec 2002 = -1.075 Datum: 1st Jan 2003 onwards = -0.925 Datum is now LAT so unlikely to change.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 22-Oct-2009
SANHO is in the process of re-evaluating and standardising all the tidal station benchmarks. Confirming their accuracy in relation to the existing national benchmark network. This process was carried out at Port Nolloth jetty resurveyed Mar.2008 new benchmark fitted mid 2009. the new benchmark is PN1 LLD +3.278m however SANHO are not completely happy with it and intend to resurvey it at some stage.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Mar-2013
On the original RLR diagram there is a comment that for the period 1973-1993 there is an anomaly of .02m between the datum values supplied. On the original diagram rlrfac was given as 6.077m. When entered onto the database the value was given as 6.057m. This value has now been used.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 15-May-2018
Port Nolloth was uninstalled due to revamping of the quayside. This is now complete and the station is scheduled to be reinstated  as soon as possible.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 07-Nov-2019
The South African Navy Hydrographic Office (SANHO) are the copyright owners of the Port Nolloth sea level data and must be contacted to request permission to use the data.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 10-Feb-2021
The South African Hydrographic Office have asked us to remove this record in line with the Hydrographic Act of 2019 (Act No. 35 of 2019) and the South African Spatial Data Infrastructure Act, 2003 (Act No. 54 of 2003). The data can be obtained directly from SANHO (email: hydrosan@iafrica.com)

