=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 16-Oct-2001
Data for 1985-95 from Dzaoudzi were obtained from a SHOM, France gauge (A.OTT type 16 float gauge) with data processed by the University of Hawaii Sea Level Center.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 14-Oct-2009
Dataset 1985-1995 replaced with revised data supplied by SHOM. Copy of previous data held in file.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 19-Oct-2009
The new gauge at Dzaoudzi has been installed at the same location as the previous gauge. The datum reference has remained the same with new benchmark F. The previous benchmark A was destroyed between 1997 and 2000. Details supplied by SHOM.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Mar-2012
The data following the gauges re-installation in 2008 looks slightly higher than previously. Because of the remote location it is difficult to confirm this.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Sep-2014
Using values from the SONEL website the latitude and longitude for Dzaoudzi have been revised.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 01-Oct-2014
Using SHOM data Dzaoudzi has been made RLR from its re-installation in 2008. Primary benchmark is N-402-BIS 7.332m above Zero Hydrographique.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 15-Jul-2025
Updated the whole dataset to ensure they include all the historical data recovered recently by SHOM and the calculated monthly and annual means match those distributed by SONEL.

