=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Ubli                280/056 RLR(1987) is 9.8m below BM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Ubli                280/056 RLR(1987) is 9.8m below BM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jan-1996
gauge destroyed 2 September 1991
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jan-1996
PRIOR TO 1990 DATA FROM AUTH 26
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-Jan-2011
According to the original RLR diagram this gauge was destroyed in 1991.

