=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-May-1995
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 17-May-1996
Revised data for 1985 received from The National Tidal Centre, Bureau of Meteorology, South Australia
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Aug-2010
Supplying authority have confirmed that tide gauge zero is LAT, and benchmark PSM 4855 is 5.037 m above LAT. RLR (2009) has been defined as 10.3 m above PSM 4855
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Feb-2021
Latest data from the NTC to download for Mourilyan Harbour is that for 2019.

