=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Split Harbour       280/031 RLR(1964) is 10.4m below BMNo165
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 04-Mar-1992
Prior to 1990 data from Hidrografski Institut, Split
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jan-1996
Tide gauge of the State Hydrographic Institute at Split
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jan-1996
Gauge=A. Ott, Kempten
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 06-Nov-1997
Split data have different datum levels either side of World War II precluding the construction of a continuous RLR time series.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-Jan-2011
No benchmark information for very early data. Very little for data for 1954. Station information sheet recently supplied refers to the gauge being operational from 1955 omwards. Primary benchmark is PN 165 3.9232m above TGZ. Benchmark R1 is 3.5051m above TGZ. RLR factor 1955 onwards is 6.477m.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 16-Jul-2019
When the 2018 data is plotted there is evidence of a surge in March 2018.

