=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 26-Aug-2010
Supplying authority has confirmed that tide gauge benchmark FSM1 is 2.438 m above TGZ RLR (2009) has been defined as 8.7 m below FSM1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 16-Mar-2016
Pohnpei C has been buddy checked with the UH gauge Pohnpei B id.1370 although the data for 2015 is not yet available the profiles compare well.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 23-Jan-2019
Many data values prior to 2010 have been revised. Because of this the complete data series has been re-loaded.

