=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-May-1995
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 17-May-1996
Revised data 1976-1990 received from the National Tidal Centre, Bureau of Meteorology, South Australia
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 18-Oct-2011
Using metadata from the National Tidal Centre, Australia this station has been made RLR. Datum is Chart Datum (CD) the TGBM does not have a name/number but is described as : Iron rail driven in to rock near the western gate to old Harbour Master's office. TGBM is 4.513m above CD. RLR factor is 5.987m.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Feb-2021
Latest data available for downland from the NTC for station Wallaroo II is that for 2019.

