=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-May-1995
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 17-May-1996
Revised data for 1985-1986 received from the National Tidal Centre, Bureau of Meteorology, South Australia
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Aug-2010
Data supplier has confirmed that tide gauge zero for datum is LAT, and benchmark H&M BM14 is 5.543 m above LAT. RLR (2009) has been defined as 10.6 m below H&M BM14
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Feb-2021
The latest data from the NTC available to download for Lucinda is that for 2019.

