=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Bodo                040/101 RLR(1964) is 10.6m below BM K13 N31
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Mar-1995
Tide gauge network modernised, new equipment installed in 1989
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Jan-2009
Following the input of revised data values station made Metric awaiting datum information.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 06-Apr-2009
2007/8 mean sea level values entered as Metric only awaiting confirmation of a datum query.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 29-Oct-2009
From the Norwegian Mapping Authoriy website it is obvious that they have revised their datasets. RLR (2008) was calculated for Bodo giving a value of 5.149m this was applied to the whole dataset. RLR (2008) is 30.2m below TGBM K13 N47. Data now looks OK although confirmation required from the Norwegian Mapping Authority. Data point for May 1970 has been 'switched off' as it is a spike. Data for this month does not appear on the Norwegian website.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Sep-2012
For information on sea level change along the Norwegian coast see paper "Contributions to sea level variability along the Norwegian coast for 1960-2010" by K. Richter, J.E.O. Nilsen and H. Drange.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 25-Jan-2018
Monthly mean values for 1989 for November and December have been updated using revised values from the Norwegian Mapping Authority.

