=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 03-Sep-1999
Acoustic gauge (Aquatrak 4100 series sensor) installed in 1998
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 25-Apr-2000
Antalya II          310/052 RLR(1992) is 7.4m below BM MAR 1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Jun-2000
New analogue chart, float gauges were installed in 1985 in 4 Turkish
stations: Antalya II, Bodrum II, Metes/Izmir and Erdek. All were
replaced by new acoustic systems in 1998-99.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Jun-2010
Antalya II is on the Eastern Mediterranean coast. The station forms part of the
Turkish Sea Level Monitoring network.Coast/Station code 310/052 id=1681.Total
dataset has been updated
by the authority. A new RLR diagram was created. RLR (2007) is 8.000m below
TGBM ANTL-1. RLR factor is 4.836m.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 23-Jul-2019
Scientists from a number of German Environmental and Geoscience Institutes have published a paper in the Journal of Geophysical Research (JGR-Oceans) describing the analysis of data from Antalya, Eastern Mediterranean. MSL data from Antalya (id.400) has been merged with Antalya II (id.1681).In the analysis ‘Metric’ data from Antalya I has been aligned with the RLR dataset from Antalya II. The paper includes the full history of the station and the data itself. View the paper at the link:-
https://doi.org/10.1029/2018JC013906


