=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Annapolis           960/080 RLR(1974) is 8.4m below BM1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 29-Jul-1993
Low values in early 1977 follow a data gap but are probably correct - for example, compare to 960/081 Baltimore. Previously this data had been flagged but because Baltimore compares well the flags have been removed.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Oct-2011
Using NOAA data the RLR diagram has been revised. Previous Primary benchmark was BM 1 now referred to as BM 1 1928. Original value was 2.957m above the gauge datum. In 1986 this value was 2.949m and in 2003 2.942m New Primary benchmark is BM 7 with a value of 2.876m in 1986 and 2.869m in 2003.

