=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Jun-1995
1992 revised, June 1995
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 03-Sep-1999
Acoustic gauge (Aquatrak 4100 series sensor) installed in 1998
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Jun-2000
New analogue chart, float gauges were installed in 1985 in 4 Turkish
stations: Antalya II, Bodrum II, Metes/Izmir and Erdek. All were
replaced by new acoustic systems in 1998-99.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Jun-2000
Bodrum II           310/046 RLR(1986) is 8.608m below BM MAR 1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 01-Jul-2010
During May 2010 the complete revised data holding from the Turkish Sea Level
Monitoring Network were supplied to the PSMSL from the General Command of
Mapping.All datasets including that for Bodrum II were replaced. Previously RLR
the values were TGBM BM MARI 3.475m above Chart Datum. RLR (1986) 8.608m below
TGBM BM MARI. RLR factor 6.0m.
A revised RLR diagram was created with Primary Benchmarl BDRM-1 2.578m above
TGZ.
RLR (2008) 8.3m below TGBM BDRM-1. RLR factor 5.722m
Add 5.722m to all data values to refer to RLR (2008).
There also exists a secondary benchmark BDRM-2. This is 2.407m above TGZ.

