=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 21-Sep-1994
Gauge was a Lege stilling well between 1956 and 1974, replaced by
a Lege or Kent 1975-1980.  A Munro stilling well gauge was installed
in February 1980.
Hilbre is an historic station last data 1983
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-Jan-2001
Recent work on vertical land movements in the UK can be found from
the University of Nottingham web site:
http://ukcogr.iessg.nottingham.ac.uk/~eosi/
1977-1979 BAD SILTATION PROBLEMS -- NOT FOR PUBLICATION
PRIOR TO 1963 VALUES BASED ON 8 READINGS/DAY.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 08-Jan-2026
1854-1903 data has been added based on data recovered by the Zooniverse UK Tides project. This new data is based on ledgers of recorded measurements read off a mareogram at 15-minute intervals. Data was recorded used a siphon water conduit to the open sea (Thomson 1876).
The ledgers report heights are given relative to Liverpool's Old Dock Sill, as with the similarly recovered data from George's Landing Pier in Liverpool, see ID 15. However, we have no information about how that datum was transferred to Hilbre, we advise treating it with suspicion as values at Hilbre are consistenly tens of centimetres lower than Liverpool, with the difference varying considerably over time.

