=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Maloy            040/211 RLR(1964) is 10.1m below BM No7
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Mar-1995
Tide gauge network modernised, new equipment installed in 1986
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Jan-2009
Following the input of revised data values station made Metric awaiting datum information.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 06-Apr-2009
2007/8 mean sea level values entered as Metric only awaiting confirmation of a datum query.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 29-Oct-2009
The Norwegian Mapping Authority have revised their datasets. Whole dataset for Maloy now refers to TGBM A29 N26 6.615m above TGZ. A RLR value for 2008 was calculated. Add 5.785 to all data to refer to RLR (2008) RLR (2008) is 12.4m below TGBM A29 N26
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 19-Apr-2010
The datapoints for 1959 and 1960 where switched off as there appears to be a datum error for this period. This data does not appear on the Norwegian website.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Sep-2012
For information on sea level rise along the Norwegian coast see paper "Contributions to sea level variability along the Norwegian coast for 1960-2010" by K. Richter, J.E.O. Nilsen and H Drange.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 15-Jul-2013
The Norwegian authority has now confirmed that the Maloy data for 1959-1960 is missing from their database. They have asked PSMSL not to display this data.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jan-2018
Using updated values from the Norwegian Mapping Authority a data value for April 1986 has been added.

