=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 26-Aug-2010
Isabela de Sagua is now RLR. BM 4507 is 1.156m above the Geodesic National Datum (GND) while TGZ is -0.62m below GND. The data is referred to TGZ. RLR factor is 5.724m.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 03-Mar-2016
To reflect the fact that the monthly means supplied refer to TGZ and not GND the RLR diagram has been redrawn. As a result the RLRFAC has changed fron 5.724m to 6.324m. RLR (2008) is now 8.1m below TGBM 04507.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 29-Jun-2016
Using recent information received from Cuba the tide gauge sensors are from 1972 a float recording hourly and from 2013 a radar with 6 minute frequency.

