=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 17-Oct-2000
Data now supplied by Service Hydrographique et Ocean. de la Marine, Brest.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 19-Oct-2000
Sete RLR(2000) is 8.775m below BM MC-J3-K3-46.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 04-Apr-2012
Previous primary benchmark MC-J3-K3-46 was destroyed in 2004. New Primary benchmark is M.EM3-39 6.422m above Zero Hydrographique and 6.125m above IGN 69.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-Oct-2014
Using data from SONEL the latitude and longitude for Sete has been updated. The data downloaded from SONEL contained many additional data points particularly for the 1990's. Because of this the whole dataset has been reloaded onto the database.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 22-Jun-2016
While entering the 2015 data to the dataset it was noted that data points for November-December 2011 had been revised.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 15-Jul-2025
Updated the whole dataset to ensure they include all the historical data recovered recently by SHOM and the calculated monthly and annual means match those distributed by SONEL.

