=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Mar-1995
tide gauge network modernised, new equipment installed in 1990
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 25-Apr-2000
Viker               040/341 RLR(1992) is 10.3m below TGBM (G37 N111)
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Sep-2012
For information of sea level rise along the Norwegian coast, see paper " Contributions to sea level variability along the Norwegian coast for 1960-2010 "by K. Richter, J.E.O. Nilsen and H. Drange.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 17-Nov-2015
The PSMSL has been notified by the Norwegian Authority that the tide gauge at Viker is sinking. The rate of sinking has been confirmed as 0.30mm/year. with the supply of the 2014 sea level data a revised dataset beginning January 1991 has been supplied. Future data will be supplied with the correction applied.

