=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Inchon              620/011 RLR(1964) is 12.5m below BM(origin point)
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 26-Feb-1993
gauge resited 1974
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jan-2001
Inchon - new gauge 1998/99, no further information as yet.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jul-2012
At the request of the data suppliers, KHOA the name of the station has been
revised to Incheon. The values for lat. and long. have also been revised.
Tide gauge is an OTT float

