=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Lowestoft           170/068 RLR(1978) is 9.6m below BM TM5477 9272
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Sep-1993
August-October 1979 datum suspect
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-Sep-1994
A Lege stilling well gauge was installed in June 1955, replace by Munro and Ott systems in separate wells in May 1970.  From February 1985 data have been taken from a potentiometer
attached to the Munro stilling well.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 17-Jul-1997
1989 - November 1996: possible error in data of 2-3mm November 1996: new gauge installed
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-Jan-2001
Recent work on vertical land movements in the UK can be found from the University of Nottingham web site: http://ukcogr.iessg.nottingham.ac.uk/~eosi/
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 03-Jul-2014
TGI visited the site 04.12.2013 for general maintenance and changed the compressor.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 18-May-2015
TGI were at site on 02.05.14 and 23.11.14 for General Maintenance.

