1955 - 1956 values based on high and low waters
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Veraval             500/021 RLR(1962) is 11.9m below GTS SBM 1955
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 04-Aug-1994
For a discussion of interannual variability of sea level along the coasts of Pakistan and India, see Clarke and Liu, Journal of Physical Oceanography, 24, 1224, 1994.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 06-Feb-2002
Veraval replaced by nearest port Porbandar in Feb. 1997, but was ravaged by cyclone in June 1998 and not yet reconstructed.  Unsure when Veraval ceased operating.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 06-Dec-2002
SMRC Newsletter Jul-Dec 2001 reports high E coast correlation with SOI and MSL. MSL is much higher during La Nina tropical cyclones than during El Nino.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 26-Jan-2016
A value of MTL-MSL=19 mm has been applied to the RLR data for the period 1955-1956. The value was derived using a historic databank of harmonic tidal constants gathered by the International Hydrographic Organization (IHO).  Care must be taken when using these IHO constants, though, as there are many known errors in tidal amplitudes and phases.

