=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Aug-1996
For discussions of MSL changes and extreme sea levels around Namibia and South Africa, see: G.B.Brundrit, S.Afr.J.Mar.Sci.,16,9-17,1995 and S.Searson and G.B.Brundrit, S.Afr.J.of Science, 91,579-588,1995.
To be disregarded - Guage on unstable jetty
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Jul-2006
Data for 2000 were supplied by BODC. The values were supplied to BODC via the University of Cape Town and so are not being classed as official.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 07-Aug-2006
Following the supply of data from the South African Hydrographic Office the data for the year 2000 has now been revised with the official values.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Sep-2009
Heights of chart datum relative to land levelling
datum in South Africa and Namibia: Saldanha
Datum: up to 31st Dec 1978 = -0.582
Datum: 1st Jan 1979 - 31st Dec 1997 = -0.900
Datum: 1st Jan 1998 - 31st Dec 2002 = -0.975
Datum: 1st Jan 2003 onwards = -0.865
Datum is now LAT so unlikely to change.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-May-2010
There appears to be a spike in the dataset for November 2002. This is possibly real as a spike during Nov/Dec 2002 appears in several of the S. African stations.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 07-Nov-2019
The South African Navy Hydrographic Office (SANHO) are the copyright owners of the Saldanha sea level data and must be contacted to request permission to use the data.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 10-Feb-2021
"The South African Hydrographic Office have asked us to remove this record in line with the Hydrographic Act of 2019 (Act No. 35 of 2019) and the South African Spatial Data Infrastructure Act, 2003 (Act No. 54 of 2003). The data can be obtained directly from SANHO (email: hydrosan@iafrica.com)

